{"text_format":"5","workbook":"ods","n_sheets":1,"sheets":["Tabelle1"],"read":"whole","date_system":"iso_in_file"}

{"sheet":"Tabelle1","index":0,"n_rows":191,"n_cols":36,"rows_kept":191,"merged":[[4,17,5,27],[4,28,4,35],[5,8,5,16],[5,28,6,28],[5,29,6,29],[5,30,5,32],[5,33,5,35]]}
[null,null,4,"LinuxCNC Latency data overview / summary"]
[]
[{"$nulls":3},"Abbreviations: nt: not tested | ?: unknown | {}: comments | RT-error: «Unexpected realtime delay on task 0 with period xxx», script aborted | dnc: data not collected (ie. Script version did not support collecting this data yet) | UD: undisclosed {script flaw?} | crossed out: Stuff not compatible w. Lcnc"]
[{"$nulls":6},"Script todos:  could not find this data {SF}"]
[{"$nulls":17},"Os / LinuxCNC data",{"$nulls":10},"Latency data"]
[{"$nulls":7},"Suitability","System data",{"$nulls":19},"Duration(s) [s]","CPU Temp [°C]","Servo [uS]",null,null,"Base [uS]"]
[{"$nulls":3},"S#","Reference \nLink","Script Version","Date","Servo | \nBase","System","BIOS","Chipset","Disc","CPU | cores","Cache [kB]","RAM [MB]","GPU","GPU driver","OS","Desktop","Windowmanager","Displaymanager","Kernel","GRUB_CMDLINE LINUX_DEFAULT","Cpu idle driver","pcspkr","snd modules","swap pre | post","LinuxCNC Version",null,null,"min [uS]","max [uS]","Std dev. [uS]","min [uS]","max [uS]","Std dev. [uS]"]
[{"$nulls":3},1,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc#172205","20200619-c","2020-06-22","Yes |\nnt","LENOVO,  10A8S1BX0N","FBKT75AUS, 04/01/2014","dnc","SSD","I5-4570 | 4c",6144,"4096, 2048","Xeon E3-1200 v3/4th Gen","i915","Linux Mint 19.3","?","?",null,"5.4.0-0.bpo.4-rt-amd64","quiet splash","intel_idle","nt","nt","8464 | 8464","2.9.0~pre0.2237.g829ce3e65",125,null,-74,85,7.7,"nt","nt","nt"]
[{"$nulls":3},2,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc#172308","20200619-b","2020-06-22","Yes | \nYes","OptiPlex 980","A04, 09/11/2010","dnc","SSD","i5 CPU 650 | 2c",4096,"2048, 2048","Interated","i915","Debian GNU/Linux 10 (buster)","KDE","? {probably sddm}",null,"4.19.0-9-rt-amd64","quiet splash intel_idle.max_cstate=0 processor.max_cstate=1 idle=poll isolcpus=1","none","nt","nt","0 |  0","2.9.0~pre0.2237.g829ce3e65",7206,null,-19.3,17.8,0.7,-19.9,17.6,0.3]
[{"$nulls":3},3,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc#172308","20200622-pre","2020-06-22","Tweaks needed","OptiPlex 980","A04, 09/11/2010","Intel Corporation 5 Series/3400","SSD","i5 CPU 650 | 2c",4096,"2048, 2048","Interated","i915","Linux Mint 19.3","Mate","?",null,"5.4.0-0.bpo.4-rt-amd64","quiet splash intel_idle.max_cstate=0 processor.max_cstate=1 idle=poll isolcpus=1","none","nt","nt","0 |  0","2.9.0~pre0.2245.g09397b8d3","164 / \nRt-error",null,-20,22,0.8,-18.1,16.9,0.8]
[{"$nulls":3},4,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc#172460","20200622-pre","2020-06-23","Yes | \nYes","OptiPlex 980","A04, 09/11/2010","Intel Corporation 5 Series/3400","SSD","i5 CPU 650 | 2c",4096,"2048, 2048","Interated","i915","Linux Mint 19.3","Mate","?",null,"4.9.0-12-rt-amd64","quiet splash intel_idle.max_cstate=0 processor.max_cstate=1 idle=poll isolcpus=1","none","nt","nt","0 |  0","2.9.0~pre0.2245.g09397b8d3",7205,null,-19.6,18.7,0.2,-26.7,26.7,0.7]
[{"$nulls":3},5,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc#172496","20200619-c","2020-06-23","Yes | \nNo","Gigabyte Technology Co., Ltd.,  P35-DS4","F14,  06/19/2009","dnc","SSD","Core(TM)2 Quad\n | 4c",4096,"2048, 2048, 2048","Cypress PRO [Radeon HD 5850]","radeon","Debian GNU/Linux 9 (stretch)","?","?",null,"4.9.0-11-rt-amd64","quiet","none","nt","nt","0 |  0","2.9.0~pre0.22","8 / 10 / \nRt-error",null,-23.6,23.3,1.2,-24.6,104,1.5]
[{"$nulls":3},6,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc#172681",20200624,"2020-06-25","Yes | \nYes","HP Compaq Elite 8300 SFF","K01 v02.90,  07/16/2013","Intel Corporation 7 Series/C216","SSD","I5-3570 | 4c",6144,"4096, 4096","Xeon E3-1200 v2/3rd","i915","Debian GNU/Linux 10 (buster)","KDE","? {probably sddm}",null,"4.19.0-9-rt-amd64","quiet splash intel_idle.max_cstate=0 processor.max_cstate=1 idle=poll isolcpus=1,2,3","none","blacklisted","loaded","0 |  0","2.9.0~pre0.2245.g09397b8d3",7200,null,-39,30.9,3.4,-31.5,34,0.6]
[{"$nulls":3},7,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc#172681",20200624,"2020-06-25","Yes | \nOmitted","HP Compaq Elite 8300 SFF","K01 v02.90,  07/16/2013","Intel Corporation 7 Series/C216","SSD","I5-3570 | 4c",6144,"4096, 4096","Xeon E3-1200 v2/3rd","i915","Debian GNU/Linux 10 (buster)","KDE","? {probably sddm}",null,"4.19.0-9-rt-amd64","quiet splash intel_idle.max_cstate=0 processor.max_cstate=1 idle=poll isolcpus=1,2,3","none","blacklisted","loaded","0 |  0","2.9.0~pre0.2245.g09397b8d3",7200,null,-63.4,60.5,3.8,"omitted","omitted","omitted"]
[{"$nulls":3},8,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=0#172695",20200624,"2020-06-25","Yes | \nYes","HP Compaq Elite 8300 SFF","K01 v02.90,  07/16/2013","Intel Corporation 7 Series/C216","SSD","I5-3570 | 4c",6144,"4096, 4096","Xeon E3-1200 v2/3rd","i915","Debian GNU/Linux 10 (buster)","KDE","? {probably sddm}",null,"4.9.0-12-rt-amd64","quiet splash intel_idle.max_cstate=0 processor.max_cstate=1 idle=poll isolcpus=1,2,3","none","blacklisted","loaded","0 |  0","2.9.0~pre0.2245.g09397b8d3",7205,null,-18,18.7,0.5,-47.2,49,0.9]
[{"$nulls":3},9,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc#172735",20200624,"2020-06-25","Yes | \nYes","HP Compaq Elite 8300 SFF","K01 v02.90,  07/16/2013","Intel Corporation 7 Series/C216","SSD","I5-3570 | 4c",6144,"4096, 4096","Xeon E3-1200 v2/3rd","i915","Debian GNU/Linux 10 (buster)","KDE","? {probably sddm}",null,"4.19.0-9-rt-amd64","quiet splash intel_idle.max_cstate=0 processor.max_cstate=1 idle=poll isolcpus=1","none","blacklisted","loaded","0 |  0","2.9.0~pre0.2245.g09397b8d3",7201,null,-28.7,26.9,0.5,-37.8,39.9,1.1]
[{"$nulls":3},10,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc#172735",20200624,"2020-06-25","Yes | \nOmitted","HP Compaq Elite 8300 SFF","K01 v02.90,  07/16/2013","Intel Corporation 7 Series/C216","SSD","I5-3570 | 4c",6144,"4096, 4096","Xeon E3-1200 v2/3rd","i915","Debian GNU/Linux 10 (buster)","KDE","? {probably sddm}",null,"4.19.0-9-rt-amd64","quiet splash intel_idle.max_cstate=0 processor.max_cstate=1 idle=poll isolcpus=1,2,3","none","blacklisted","loaded","0 |  0","2.9.0~pre0.2245.g09397b8d3",7205,null,-72.8,68.9,3.1,"omitted","omitted","omitted"]
[{"$nulls":3},11,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=10#172788",20200624,"2020-06-26","No |\nNo","ASUS AT5MNI","0214 12/01/2009","?","SSD","Atom(TM) CPU D510 | 2c",512,"1024, 1024","Atom Processor D4xx/D5xx/N4xx/N5xx","i915","Debian GNU/Linux 10 (buster)","KDE","? {probably sddm}",null,"4.9.0-12-rt-amd64","quiet splash intel_idle.max_cstate=0 processor.max_cstate=1 idle=poll isolcpus=1","none","blacklisted","blacklisted","0 |  0","2.9.0~pre0.2258.gc90c1926d","15 /  \nRt-error",null,-93.7,121,3.5,-57.2,59.6,4.3]
[{"$nulls":3},12,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=10#172802",20200624,"2020-06-26","Yes | \nNo parport","FUJITSU,  ESPRIMO Q920","V4.6.5.4 R1.37.0 for D3233-A1x,  08/06/2015","Intel Corporation 8 Series","SSD","i7-4765T |\n4c",8192,"8192, 8192","Xeon E3-1200 v3/4th Gen","i915","Debian GNU/Linux 10 (buster)","KDE","? {probably sddm}",null,"4.9.0-12-rt-amd64","quiet splash intel_idle.max_cstate=0 processor.max_cstate=1 idle=poll isolcpus=1","none","blacklisted","blacklisted","0 |  0","2.9.0~pre0.2258.gc90c1926d",7201,null,-34.7,37.3,2.8,"no parport","no parport","no parport"]
[{"$nulls":3},13,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=10#179589",20200624,"2020-08-26","Yes | \nNo parport","HP Compaq Elite 8300 USDT","K01 v02.05,  05/07/2012","Intel Corporation 7 Series/C216","SSD","i5-3470S | 4c",6144,"4096, 4096","Xeon E3-1200 v2/3rd Gen","i915","Linux Mint 20","?","?",null,"4.9.0-13-rt-amd64","quiet splash","intel_idle","blacklisted","loaded","0 |  0","2.9.0~pre0.2662.g3039a67a6",720,null,-93.1,105.7,9.6,"no parport","no parport","no parport"]
[{"$nulls":3},14,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=10#179602",20200624,"2020-08-26","? | \n?","Itautec S.A., Infoway","0110,  03/02/2009","UD","rotational","Core(TM)2 Duo CPU E7500 | 1c",3072,"1024, 1024","?","?","Linux Mint 19.3","?","?",null,"5.4.0-0.bpo.4-rt-amd64","quiet splash","none","blacklisted","blacklisted","16732 |  27432","2.8.0~pre3.31.gb7c7ab5aa","23 / RT-error",null,-39.8,52.1,4.4,-24.9,74.6,2.6]
[{"$nulls":3},15,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=30#179847",20200624,"2020-08-28","? | \n?","Itautec S.A., Infoway","0110,  03/02/2009","UD","rotational","Core(TM)2 Duo CPU E7500 | 1c",3072,"2048, 2048","?","?","Linux Mint 19.3","?","?",null,"5.4.0-0.bpo.4-rt-amd64","quiet splash","none","blacklisted","blacklisted","0 |  0","2.8.0~pre3.31.gb7c7ab5aa","12 / RT-error",null,-24.8,51.7,2,-22.3,22.8,7.5]
[{"$nulls":3},16,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=30#179989",20200624,"2020-08-28","Yes |\nnt","ECS,  BAT-I","5.6.5,  01/18/2016","UD","SSD","Celeron(R) CPU  J1800",1024,8192,"Atom Processor Z36xxx/Z37xxx","i915","Linux Mint 20","?","?",null,"4.9.0-13-rt-amd64","quiet isolcpus=1 splash","intel_idle","blacklisted","blacklisted","0 |  0","2.8.0~pre3.50.g2fe8ba3c9",7201,null,-57.7,64.3,6.2,"nt","nt","nt"]
[{"$nulls":3},17,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=40#180536",20200624,"2020-09-03","Yes | \nYes","Dell Inc.,  Precision WorkStation T3500","A17, 05/28/2013","UD","rotational","Xeon(R) CPU  W3565",8192,"2048, 2048, 2048","GF106GL [Quadro 2000]","nouveau","Linux Mint 20","?","?",null,"4.9.0-13-rt-amd64","quiet splash","intel_idle","blacklisted","loaded","0 |  0","2.8.0.4.g4dc48a252",7200,null,-21.1,20.7,0.8,-20,20.3,0.5]
[{"$nulls":3},18,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=40#180684","20200903pre","2020-09-04","No {Kernel?} | \nNo parport","FUJITSU,  ESPRIMO_D956","V5.0.0.11 R1.4.0 for D3432-A1x,  10/08/2015","UD","SSD","I7-6700 \n| 1c {?????}",8192,"4096, 4096","HD Graphics 530","i915","Debian GNU/Linux 10 (buster)","KDE","? {probably sddm}",null,"4.9.0-12-rt-amd64","quiet splash","intel_idle","blacklisted","blacklisted","0 |  0","2.9.0~pre0.2740.gcb1425e5d",7202,null,-450.8,448.6,7.3,"no parport","no parport","no parport"]
[{"$nulls":3},19,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=40#180798",20200905,"2020-09-05","No |\nNo","LENOVO,  0674GEG {z61p}","7FETA9WW (2.27 ),  08/26/2009","UD","SSD","Core(TM)2 CPU T7200",4096,"2048, 2048","?","?","Linux Mint 19.3","Mate","?",null,"4.9.0-12-rt-amd64","quiet splash intel_idle.max_cstate=0 processor.max_cstate=1 idle=poll isolcpus=1","none","blacklisted","blacklisted","0 |  0","2.9.0~pre0.2747.gb86438619","128 | \nRt-error",null,-878.5,878.8,3.7,"no parport","no parport","no parport"]
[{"$nulls":3},20,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=40#181151",20200624,"2020-09-07","Yes |\nnt","K4-I5-4200U Aliexpress","5.011, 07/31/2019","UD","SSD","i5-4200U",3072,8192,"Haswell-ULT","i915","Debian GNU/Linux 10 (buster)","?","?",null,"4.19.0-10-rt-amd64","quiet splash intel_idle.max_cstate=0 processor.max_cstate=1 idle=poll isolcpus=1","none","blacklisted","blacklisted","0 |  0","2.9.0~pre0.2747.gb86438619",7204,null,-60.3,68.4,7.9,"nt","nt","nt"]
[{"$nulls":3},21,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=50#182603",20200905,"2020-09-15","Yes | \nYes","OptiPlex 980","A18, dated 02/27/2018","Intel Corporation 5 Series/3400","SSD","I5 750 |\n4c",8192,"2048, 2048,  2048, 2048","RV710 [Radeon HD 4550]","radeon","Debian GNU/Linux 10 (buster)","KDE","? {probably sddm}",null,"4.19.0-10-rt-amd64","quiet splash idle=poll","none","blacklisted","blacklisted","0 |  0","2.9.0~pre0.2800.g470fce12e",7204,null,-11.9,14.2,1.6,-18.4,19.4,0.9]
[{"$nulls":3},22,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=60#183625",20200922,"2020-09-22","Probably not |\nnt","LENOVO,  3254CTO {Edge 340 Laptop}","H0ET98WW (2.58 ),  08/18/2016","Intel Corporation 7 Series/C216","rotational","i5-3210M | \n1c {Multi core off?}",3072,4096,"3rd Gen Core processor Graphics Controller","i915","Linux Mint 19.3","?","?",null,"4.19.106-rt46-lcnc","quiet splash","intel_idle","blacklisted","blacklisted","0 |  0","2.8.0.39.g76260b4f7",7202,null,-197.8,192.9,4.7,"no parport","no parport","no parport"]
[{"$nulls":3},23,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=70#183735",20200922,"2020-09-25","No  | \nNo parport","LENOVO,  2241BM7 {T500 laptop}","6FET92WW (3.22 ),  12/14/2011","Intel Corporation Mobile 4 Series","SSD","Core(TM)2 Duo CPU  P8600 | 2c",3072,"2048, 2048","Mobile 4 Series Chipset Integrated Graphics Controller","i915","Debian GNU/Linux 10 (buster)","?","Xfwm4",null,"4.19.106-rt46-lcnc","quiet splash isolcpus=3","acpi_idle","blacklisted","blacklisted","0 |  0","2.8.0",7202,null,-431.1,428.8,3.2,"no parport","no parport","no parport"]
[{"$nulls":3},24,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=70#183894",20200922,"2020-09-24","Probably not |\nnt","LENOVO,  3254CTO {Edge 340 Laptop}","H0ET98WW (2.58 ),  08/18/2016","Intel Corporation 7 Series/C216","rotational","i5-3210M | \n1c {Multi core off?}",3072,4096,"3rd Gen Core processor Graphics Controller","i915","Linux Mint 20","?","?",null,"4.9.0-13-rt-amd64","quiet splash","intel_idle","blacklisted","blacklisted","0 |  0","2.8.0.39.g76260b4f7",7200,null,-223.2,212.4,12.1,"no parport","no parport","no parport"]
[{"$nulls":3},25,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=80#184003",20200922,"2020-09-26","Yes | \nNo parport","LENOVO,  3254CTO {Edge 340 Laptop}","H0ET98WW (2.58 ),  08/18/2016","Intel Corporation 7 Series/C216","rotational","i5-3210M | \n1c {Multi core off?}",3072,4096,"3rd Gen Core processor Graphics Controller","i915","Debian GNU/Linux 10 (buster)","?","?",null,"4.19.0-10-rt-amd64","quiet","intel_idle","loaded","loaded","0 |  0","2.8.0",7199,null,-90.8,98.4,2.5,"no parport","no parport","no parport"]
[{"$nulls":3},26,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=80#184021",20200922,"2020-09-26","Probably not |\nnt","LENOVO,  3254CTO {Edge 340 Laptop}","H0ET98WW (2.58 ),  08/18/2016","Intel Corporation 7 Series/C216","SSD","i5-3210M | \n1c {Multi core off?}",3072,4096,"3rd Gen Core processor Graphics Controller","i915","Debian GNU/Linux 10 (buster)","?","?",null,"4.19.0-10-rt-amd64","quiet","intel_idle","loaded","loaded","0 |  0","2.8.0",7203,null,-173.4,167.9,7.7,"no parport","no parport","no parport"]
[{"$nulls":3},27,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=80#184048",20200922,"2020-09-26","Probably Yes | \nNo parport","RPi4 4GB","?","UD","SSD","ARMv7 Processor rev 3","?","? {4096}","?","?","Raspbian GNU/Linux 10 (buster)","?","?",null,"4.19.71-rt24-v7l+","?","?","blacklisted","blacklisted","0 |  0","2.8.0",7203,null,-126.9,146.9,2.6,"no parport","no parport","no parport"]
[{"$nulls":3},28,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=90#184089",20200922,"2020-09-27","Yes |\nnt","ECS,  BAT-I","5.6.5, dated 01/18/2016","UD","SSD","Celeron(R) CPU  J1800 | 2c",1024,8192,"Atom Processor Z36xxx/Z37xxx","i915","Linux Mint 20","?","?",null,"4.9.0-13-rt-amd64","quiet isolcpus=1 splash","intel_idle","blacklisted","blacklisted","0 |  0","2.8.0.45.g6319aa042",7203,null,-64.2,82.8,0.3,"nt","nt","nt"]
[{"$nulls":3},29,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=90#184117",20200922,"2020-09-28","Probably not |\nnt","LENOVO,  4157CTO {T530 laptop}","60KT45AUS,  03/30/2012","Intel Corporation 5520/5500/X58 ","SSD","Xeon(R) CPU           W3550 | 4c",8192,"4096, 4096, 4096, 4096, 4096, 4096","GF106GL [Quadro 2000]","nouveau","Linux Mint 19.2","?","?",null,"4.19.106-rt46-lcnc","quiet splash","intel_idle","blacklisted","blacklisted","0 |  0","2.8.0.44.gad1491d89","27 | \n{Rt-error?}",null,-11.9,13.6,1.6,"no parport","no parport","no parport"]
[{"$nulls":3},30,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=110#184283",20200922,"2020-09-29","No |\nNo","OptiPlex FX160","A13,  01/19/2012","UD","SSD","Atom(TM) CPU  330 ",512,"2048, 2048","771/671 PCIE VGA","?","Debian GNU/Linux 10 (buster)","?","Xfwm4",null,"4.9.0-12-rt-amd64","quiet splash","intel_idle","blacklisted","blacklisted","0 |  0","2.8.0",7202,null,-396.4,400.8,16.1,"no parport","no parport","no parport"]
[{"$nulls":3},31,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=110#184367",20200922,"2020-09-29","Yes | \nNo parport","Lenovo 20EGS01900\nThinkpad W541\n","GNET79WW (2.27 ),  03/16/2016","Intel Corporation 8 Series/C220","SSD","i7-4810MQ | 4c",6144,"8192, 8192","GK106GLM [Quadro K2100M]\n4th Gen Core Processor Integrated Graphics","nouveau\nI925","Debian GNU/Linux 10 (buster)","?","Xfwm4",null,"4.9.0-12-rt-amd64","quiet splash","intel_idle","blacklisted","loaded","0 |  0","2.8.0",7199,null,-56,54.5,4.3,"no parport","no parport","no parport"]
[{"$nulls":3},32,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=110#184500",20200930,"2020-10-01","Yes | \nYes","OptiPlex 980","A05,  11/03/2010","Intel Corporation 5 Series/3400","SSD","i7 CPU 870 |\n4c",8192,"2048, 2048, 2048, 2048","RV710 [Radeon HD 4550]","radeon","Debian GNU/Linux 10 (buster)","Kde","Kwin","sddm","4.19.0-11-rt-amd64","quiet splash isolcpus=3","intel_idle","blacklisted","blacklisted","0 |  0","2.8.0",7204,null,-11.9,11.7,0.3,-16.1,16,3.2]
[{"$nulls":3},33,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=110#184500",20200930,"2020-10-01","No | \nNo {GPU!!!}","OptiPlex 980","A05,  11/03/2010","Intel Corporation 5 Series/3400","SSD","i7 CPU 870 |\n4c",8192,"2048, 2048, 2048, 2048","RV620 LE [Radeon HD 3450]","radeon","Debian GNU/Linux 10 (buster)","Kde","Kwin","sddm","4.19.0-11-rt-amd64","quiet splash isolcpus=3","intel_idle","blacklisted","blacklisted","0 |  0","2.8.0","52 | \nRt-error",null,-3.5,4.1,0.1,-44.8,45.8,0.3]
[{"$nulls":3},34,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=120#184528",20200930,"2020-10-01","Yes | \nNo parport","LENOVO,  3254CTO {Edge 340 Laptop}","H0ET98WW (2.58 ),  08/18/2016","Intel Corporation 7 Series/C216","SSD","i5-3210M | \n1c {Multi core off?}",3072,"8192, 8192","3rd Gen Core processor Graphics Controller","i915","Linux Mint 19.3","lightdm","Xfwm4","lightdm","4.19.106-rt46-lcnc","quiet","intel_idle","blacklisted","blacklisted","0 |  0","2.8.0",7203,null,-113.8,121,5.9,"no parport","no parport","no parport"]
[{"$nulls":3},35,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=120#185014",20200930,"2020-10-05","Yes | \nNo parport","LENOVO,  3254CTO {Edge 340 Laptop}","H0ET98WW (2.58 ),  08/18/2016","Intel Corporation 7 Series/C216","SSD\n{new one}","i5-3210M | \n1c {Multi core off?}",3072,"8192, 8192","3rd Gen Core processor Graphics Controller","i915","Debian GNU/Linux 10 (buster)","lightdm","Xfwm4","lightdm","4.19.0-10-rt-amd64","quiet","intel_idle","blacklisted","blacklisted","0 |  0","2.8.0",7202,null,-73.9,73.7,5.1,"no parport","no parport","no parport"]
[{"$nulls":3},36,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=120#185033",20200930,"2020-10-05","Yes | \nNo parport","LENOVO,  3254CTO {Edge 340 Laptop}","H0ET98WW (2.58 ),  08/18/2016","Intel Corporation 7 Series/C216","rotational","i5-3210M | \n1c {Multi core off?}",3072,"8192, 8192","3rd Gen Core processor Graphics Controller","i915","Debian GNU/Linux 10 (buster)","lightdm","Xfwm4","lightdm","4.19.0-10-rt-amd64","quiet","intel_idle","blacklisted","blacklisted","0 |  0","2.8.0",7201,null,-55.4,55.1,3.3,"no parport","no parport","no parport"]
[{"$nulls":3},37,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=130#185271",20200930,"2020-10-06","Yes | \nNo parport","Supermicro,  Super Server","1.2a,  02/20/2020","Intel Corporation Q370","SSD","Pentium(R) Gold G5420",4096,"16384, 16384","Intel Corporation","i915","Debian GNU/Linux 10 (buster)","xfce4","Xfwm4","lightdm","4.19.0-10-rt-amd64","quiet","intel_idle","blacklisted","blacklisted","0 |  0","2.8.0",7201,null,-80.2,82.6,5.3,"no parport","no parport","no parport"]
[{"$nulls":3},38,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=130#185297",20200930,"2020-10-07","Yes | \nNo parport","Supermicro,  Super Server","1.2a,  02/20/2020","Intel Corporation Q370","SSD","Pentium(R) Gold G5420",4096,"16384, 16384","Intel Corporation","i915","Linux Mint 19.3","lightdm","Xfwm4","lightdm","4.19.106-rt46-lcnc","quiet","intel_idle","blacklisted","blacklisted","0 |  0","2.8.0",7201,null,-57.6,60.7,2,"no parport","no parport","no parport"]
[{"$nulls":3},39,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=130#185312",20200930,"2020-10-07","Yes | \nNo parport","Supermicro,  Super Server","1.2a,  02/20/2020","Intel Corporation Q370","SSD {added M.2 SSD, now 2 ssds?}","Pentium(R) Gold G5420",4096,"16384, 16384","Intel Corporation","i915","Linux Mint 19.3","lightdm","Xfwm4","lightdm","4.19.106-rt46-lcnc","quiet","intel_idle","blacklisted","blacklisted","0 |  0","2.8.0",7202,null,-76.1,79.2,5.3,"no parport","no parport","no parport"]
[{"$nulls":3},40,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=140#185688","20201003pre","2020-10-11","No |\nNo","LENOVO,  2774AP3\n{x301 laptop}","6EET52WW (3.12 ),  08/10/2010","Intel Corporation Mobile 4 Series","SSD","Core(TM)2 Duo CPU     U9400\n| 2c",3072,"2048, 2048","Mobile 4 Series Chipset Integrated Graphics Controller","i915","Debian GNU/Linux 10 (buster)","kdeinit5","Kwin","sddm","4.19.0-11-rt-amd64","quiet","acpi_idle","blacklisted","blacklisted","0 |  0","2.8.0",7201,null,-523,518.1,4.1,"no parport","no parport","no parport"]
[{"$nulls":3},41,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=140#185724","20201003pre","2020-10-11","Probably not |\nNo parport","LENOVO,  20AV006BMZ\n{L540 laptop}","J4ET88WW(1.88),  07/20/2017","Intel Corporation 8 Series/C220","SSD","i5-4210M |\n2c\n",3072,"4096, 4096","4th Gen Core Processor Integrated Graphics","i915","Debian GNU/Linux 10 (buster)","kdeinit5","Kwin","sddm","4.19.0-11-rt-amd64","quiet","intel_idle","blacklisted","blacklisted","0 |  0","2.8.0",7202,null,-100.4,102.1,7,"no parport","no parport","no parport"]
[{"$nulls":3},42,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=140#185724","20201003pre","2020-10-11","Probably not |\nYes","LENOVO,  20AV006BMZ\n{L540 laptop}","J4ET88WW(1.88),  07/20/2017","Intel Corporation 8 Series/C220","SSD","i5-4210M |\n2c\n",3072,"4096, 4096","4th Gen Core Processor Integrated Graphics","i915","Debian GNU/Linux 10 (buster)","kdeinit5","Kwin","sddm","4.19.0-11-rt-amd64","quiet","intel_idle","blacklisted","blacklisted","0 |  0","2.8.0",7202,null,-65.4,61.5,3.4,-45.2,46.1,3.1]
[{"$nulls":3},43,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=140#185849","20201003pre","2020-10-12","No | \nNo parport","LENOVO,  2758MKG\n{W700DS Laptop}","7ZETB0WW (2.10 ),  02/08/2010","Intel Corporation Mobile 4 Series","SSD","Core(TM)2 Quad  CPU   Q9000",3072,"4096, 4096","G92GLM [Quadro FX 3700M]","nouveau","Debian GNU/Linux 10 (buster)","kdeinit5","Kwin","sddm","4.19.0-11-rt-amd64","quiet idle=poll isolcpus=2,3","intel_idle","blacklisted","blacklisted","0 |  0","2.8.0",7204,null,-408,408.5,0.3,"no parport","no parport","no parport"]
[{"$nulls":3},44,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=140#186230",20200930,"2020-10-15","No USB Eth | \nNo parport","Hewlett-Packard,  HP Elite x2 1011 G1 Tablet","M72 Ver. 01.22,  04/12/2018","UD","SSD","Core(TM) M-5Y10c",4096,"2048, 2048","HD Graphics 5300","i915","Linux Mint 19.3","gnome","Metacity (Marco)","lightdm","4.9.0-13-rt-amd64","quiet splash","intel_idle","blacklisted","loaded","0 |  0","2.9.0~pre0.2883.g6b8e03051",724,null,-235.2,260.9,13.2,"no parport","no parport","no parport"]
[{"$nulls":3},45,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=150#186419",20200930,"2020-10-18","Yes | \nNo parport","Gigabyte Technology Co., Ltd.,  B460MD3H","F2,  04/13/2020","UD","SSD","Pentium(R) Gold G6400",4096,"4096, 4096","Advanced Micro Devices, Inc. [AMD/ATI]","amdgpu","Debian GNU/Linux 10 (buster)","xfce4","Xfwm4","lightdm","4.19.0-11-rt-amd64","quiet","none","blacklisted","loaded","0 |  0","2.8.0",7202,null,-10.6,12.5,1.3,"no parport","no parport","no parport"]
[{"$nulls":3},46,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=160#187837",20200930,"2020-10-29","No {Kernel!} | No","OptiPlex 7010","A29, dated 06/28/2018","Intel Corporation 7 Series/C216","SSD","I5-3570 | 4c",6144,"4096, 4096","Xeon E3-1200 v2/3rd Gen","i915","Linux Mint 19.3","lightdm","Xfwm4","lightdm","5.0.0-32-generic","quiet splash","intel_idle","blacklisted","loaded","0 |  0"," 2.8.0.96.g589db060d",299,null,-999.6,8653.7,7.4,"no parport","no parport","no parport"]
[{"$nulls":3},47,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=160#187851",20200930,"2020-10-30","Yes | \nNo parport","OptiPlex 7010","A29, dated 06/28/2018","Intel Corporation 7 Series/C216","SSD","I5-3570 | 4c",6144,"4096, 4096","Xeon E3-1200 v2/3rd Gen","i915","Debian GNU/Linux 10 (buster)","xfce4","Xfwm4","lightdm","4.19.0-11-rt-amd64","quiet","intel_idle","blacklisted","loaded","0 |  0","2.8.0",7201,null,-82.9,69.6,3.2,"no parport","no parport","no parport"]
[{"$nulls":3},48,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=180#188008",20200930,"2020-11-01","No | \nNo parport","LENOVO,  H215, Idea center","D2KT25BUS, dated 08/18/2010","UD","SSD","AMD Athlon(tm) II X2 250",1024,"2048, 2048","RS780L [Radeon 3000]","radeon","Linux Mint 19.3","lightdm","Xfwm4","lightdm","4.19.106-rt46-lcnc","quiet splash","none","blacklisted","loaded","2556 | 2600","2.8.0.96.g589db060d",303,null,-345.7,262,11,"no parport","no parport","no parport"]
[{"$nulls":3},49,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=180#189570",20200930,"2020-11-06","Yes | \nNo parport","LENOVO,  H215, Idea center","D2KT25BUS, dated 08/18/2010","UD","SSD","AMD Athlon(tm) II X2 250",1024,"2048, 2048","RS780L [Radeon 3000]","radeon","Debian GNU/Linux 10 (buster)","xfce4","Xfwm4","lightdm","4.19.0-11-rt-amd64","quiet","none","blacklisted","loaded","2556 | 2600","2.8.0.96.g589db060d",305,null,-66.1,67,13.2,"no parport","no parport","no parport"]
[{"$nulls":3},50,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=190#190354",20200930,"2020-11-26","??\nScript error","OptiPlex 7010 USFF","A23, dated 08/09/2016","Intel Corporation 7 Series/C216","SSD","i5-3470S | 4c",6144,"4096, 4096","Xeon E3-1200 v2/3rd Gen","i915","Linux Mint 20","gnome","Metacity (Marco)","lightdm","4.9.0-13-rt-amd64","quiet splash","intel_idle","blacklisted","loaded","648, running: 772","2.8.0.124.g4501e6d67","??",73,"??","??","??","no parport","no parport","no parport"]
[{"$nulls":3},51,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=190#190397",20200930,"2020-11-27","Yes | \nNo parport","OptiPlex 7010 USFF","A23, dated 08/09/2016","Intel Corporation 7 Series/C216","SSD","i5-3470S | 4c",6144,"4096, 4096","Xeon E3-1200 v2/3rd Gen","i915","Linux Mint 20","gnome","Metacity (Marco)","lightdm","4.9.0-13-rt-amd64","quiet splash","intel_idle","blacklisted","loaded","648, running: 772","2.8.0.124.g4501e6d67",7202,34,-41.3,41.5,3,"no parport","no parport","no parport"]
[{"$nulls":3},52,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=190#190567",20200930,"2020-11-29","Yes very short test | \nNo parport","Gigabyte Technology Co., Ltd.,  X570 AORUS ELITE","F11, dated 12/06/2019","UD","SSD","Ryzen 5 3500X 6-Core",512,"4096, 4096","Ellesmere [Radeon RX 470/480/570/570X/580/580X/590]","amdgpu","Linux Mint 20","gnome","Metacity (Marco)","lightdm","4.9.0-13-rt-amd64","quiet splash","acpi_idle","blacklisted","loaded","0 |  0","2.9.0~pre0.3030.g742c3e294",124,"UD",-17.6,15.9,1.6,"no parport","no parport","no parport"]
[{"$nulls":3},53,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=200#191033",20200930,"2020-12-04","Yes | \nYes","OptiPlex 780 ","A08, dated 01/21/2011","Intel Corporation 4 Series","rotational","Core(TM)2 Duo CPU     E8400 | 1c",6144,2048,"4 Series Chipset Integrated Graphics Controller","i915","Linux Mint 19.3","lightdm","Xfwm4","lightdm","4.19.106-rt44-lcnc","quiet splash","none","blacklisted","blacklisted","0 |  0","2.8.1.1.g5d082d148",7202,30,-37.8,35.5,1.6,-31.8,32.8,4.8]
[{"$nulls":3},54,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=210#191209",20200930,"2020-12-06","Yes | \nYes","ASRock,  To Be Filled By O.E.M.","P1.90, dated 05/21/2018","UD","SSD","Intel(R) Celeron(R) CPU J3355",1024,"4096, ","UD\n{probably chipset gpu?}","i915","Debian GNU/Linux 10 (buster)","xfce4","Xfwm4","lightdm","4.19.0-13-rt-amd64","quiet isolcpus=1 splash","intel_idle","blacklisted","blacklisted","0 |  0","2.8.1.1.g5d082d148",7201,46,-21.8,21.8,0.4,-25,25.6,0.5]
[{"$nulls":3},55,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=210#191261",20200930,"2020-12-06","Yes | \nYes {prob. Too good to be true}","ASRock,  To Be Filled By O.E.M.","P1.90, dated 05/21/2018","UD","SSD","Intel(R) Celeron(R) CPU J3355",1024,"4096, ","UD\n{probably chipset gpu?}","i915","Debian GNU/Linux 10 (buster)","xfce4","Xfwm4","lightdm","4.19.0-13-rt-amd64","quiet isolcpus=1 splash","intel_idle","blacklisted","blacklisted","0 |  0","2.8.1",7205,41,-4.8,4.8,0.3,-5.4,5.5,0.3]
[{"$nulls":3},56,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=210#191481",20200930,"2020-12-09","Yes | \nYes {prob. Too good to be true}","UD","UD","UD","SSD","Celeron(R) CPU J3455 | 4c",1024,"UD","Caicos [Radeon HD 6450/7450/8450 / R5 230 OEM]","i915 \nRadeon","Debian GNU/Linux 10 (buster)","xfce4","Xfwm4","lightdm","4.19.152-rtai-amd64","quiet isolcpus=2,3 idle=poll acpi_irq_nobalance noirqbalance lapic intel_idle.maxcstate=0 processor.max_cstate=0 ipv6.disable=1 pci=routeirq","UD","blacklisted","blacklisted","0 |  0","UD",7204,42,-3.7,3.8,0.1,-4.7,4.6,0.1]
[{"$nulls":3},57,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=210#193142",20200930,"2020-12-24","Yes | \nNo parport","HP Compaq Pro 6300 SFF","K01 v02.90, dated 07/16/2013","Intel Corporation 7 Series/C216","SSD","Core(TM) i7-3770 CPU @ 3.40GHz\n| 1c {?}",8192,"4096, 4096, 4096, 4096","Xeon E3-1200 v2/3rd Gen","i915","Linux Mint 20","gnome","Metacity (Marco)","lightdm","4.9.0-13-rt-amd64","quiet splash","intel_idle","blacklisted","loaded","0 |  0","2.8.1.13.ga22256354",7200,42,-37.3,24.5,2.2,"no parport","no parport","no parport"]
[{"$nulls":3},58,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=220#193389",20200930,"2020-12-28","Yes | \nNo parport","Dell Inc.,  OptiPlex 9010","A13, dated 03/27/2013","Intel Corporation 7 Series/C216","rotational","Core(TM) i5-3570 | \n4c",6144,"2048, 2048","Xeon E3-1200 v2/3rd Gen","i915","Debian GNU/Linux 10 (buster)","xfce4","Xfwm4","lightdm","4.19.0-11-rt-amd64","quiet","intel_idle","loaded","blacklisted","0 |  0","2.8.1",7202,57,-75.7,74.3,2.9,"no parport","no parport","no parport"]
[{"$nulls":3},59,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=220#193389",20200930,"2020-12-28","Yes | \nNo parport","Dell Inc.,  OptiPlex 9010","A13, dated 03/27/2013","Intel Corporation 7 Series/C216","rotational","Core(TM) i5-3570 | \n4c",6144,"2048, 2048","Xeon E3-1200 v2/3rd Gen","i915","Linux Mint 19.2","gnome","Metacity (Marco)","lightdm","4.16.12-rt5-kona-rt","quiet splash","intel_idle","blacklisted","blacklisted","0 |  0","2.8.0~pre1",7202,60,-96.2,102,6.1,"no parport","no parport","no parport"]
[{"$nulls":3},60,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=220#193787",20200930,"2021-01-01","Yes | \nNo parport","Dell Inc.,  OptiPlex 9020","A05, dated 12/05/2013","Intel Corporation 8 Series/C220","SSD","Core(TM) i5-4670 | \n4c",6144,"4096, 4096","Xeon E3-1200 v3/4th Gen","i915","Debian GNU/Linux 10 (buster)","xfce4","Xfwm4","lightdm","4.19.0-11-rt-amd64","quiet","intel_idle","loaded","loaded","0 |  0","2.8.1",7200,75,-65.3,65.6,2.7,"no parport","no parport","no parport"]
[{"$nulls":3},60,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=220#193787",20200930,"2021-01-01","Yes | \nNo parport","Dell Inc.,  OptiPlex 9020","A05, dated 12/05/2013","Intel Corporation 8 Series/C220","SSD","Core(TM) i5-4670 | \n4c",6144,"4096, 4096","Xeon E3-1200 v3/4th Gen","i915","Debian GNU/Linux 10 (buster)","xfce4","Xfwm4","lightdm","4.19.0-11-rt-amd64","quiet","intel_idle","blacklisted","blacklisted","0 |  0","2.8.1",7200,74,-38.2,43.5,2.2,"no parport","no parport","no parport"]
[{"$nulls":3},60,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=220#193787",20200930,"2021-01-02","Yes | \nNo parport","Dell Inc.,  OptiPlex 9020","A05, dated 12/05/2013","Intel Corporation 8 Series/C220","SSD","Core(TM) i5-4670 | \n4c",6144,"4096, 4096","Oland [Radeon HD 8570 / R7 240/340 OEM]","radeon","Debian GNU/Linux 10 (buster)","xfce4","Xfwm4","lightdm","4.19.0-11-rt-amd64","quiet","intel_idle","blacklisted","blacklisted","0 |  0","2.8.1",7200,75,-45.2,49.3,1.9,"no parport","no parport","no parport"]
[{"$nulls":3},63,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=230#197489",20200930,"2021-02-02","Yes | \nNo parport","Dell Inc.,  OptiPlex 7010","A29, dated 06/28/2018","Intel Corporation 7 Series/C216 ","SSD","Core(TM) i5-3470 |\n1c {multicore disabled in bios}",6144,"4096, 4096","Xeon E3-1200 v2/3rd Gen","i915","Debian GNU/Linux 10 (buster)","gnome","Metacity (Marco)","lightdm","4.14.174-rtai-amd64","quiet splash resume=UUID=c1b3a866-389a-48fa-8427-972a3ab4953d","UD","loaded","loaded","0 |  0","UD",7204,53,18.6,20.2,2,"no parport","no parport","no parport"]
[{"$nulls":3},64,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=230#198736",20200930,"2021-02-13","Yes | \nNo parport","LENOVO,  10AAS3VA00 M93p","FBKTD8AUS, dated 09/17/2019","Intel Corporation 8 Series/C220","SSD","Core(TM) i5-4590T | \n4c",6144,"4096, 4096","Xeon E3-1200 v3/4th Gen","i915","Debian GNU/Linux 10 (buster)","xfce4","Xfwm4","lightdm","4.19.0-14-rt-amd64","quiet","intel_idle","loaded","loaded","0 |  0","2.9.0~pre0.3532.gf6440b18b",7200,71,-45.7,47.6,3.7,"no parport","no parport","no parport"]
[{"$nulls":3},65,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=240#206998",20200930,"2021-04-25","Yes | \nNo parport","HP t610 WW Thin Client","K30 v01.10, dated 10/26/2012","UD","SSD","AMD G-T56N Processor | \n2c",512,"2048, 2048","Wrestler [Radeon HD 6320]","radeon","Linux Mint 19.3","xfce4","Xfwm4","lightdm","4.19.0-16-rt-amd64","BOOT_IMAGE=/boot/vmlinuz-4.19.0-16-rt-amd64 root=UUID=4940ea09-ddf8-4575-9fb5-d7823eabf836 ro intel_idle.max_cstate=0 processor.max_cstate=0 isolcpus=1 noirqbalance","none","blacklisted","blacklisted","0 |  0","2.9.0~pre0.3844.g2e75b091a",7203,"SF",-34.3,34.8,1.1,"no parport","no parport","no parport"]
[{"$nulls":3},66,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=240#207941",20200930,"2021-05-05","Yes | \nNo parport","Acer           ,  Aspire 5740 \n{laptop}","V1.28, dated 08/12/2010","Intel Corporation 5 Series/3400 Series ","rotational","Core(TM) i3 CPU       M 330 | \n2c",3072,"2048, 2048","Park [Mobility Radeon HD 5430/5450/5470]","radeon","Linux Mint 19.3","xfce4","Xfwm4","lightdm","4.19.0-16-rt-amd64","BOOT_IMAGE=/boot/vmlinuz-4.19.0-16-rt-amd64 root=UUID=a64fe372-f54e-4239-93e4-fd10dc0959cc ro intel_idle.max_cstate=0 processor.max_cstate=0 isolcpus=1 noirqbalance noht","none","blacklisted","blacklisted","0 |  0","2.9.0~pre0.3864.g922749755",3600,80,-44.4,44.3,5,"no parport","no parport","no parport"]
[{"$nulls":3},67,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=240#211211",20200930,"2021-06-05","Yes | \nNo parport","Dell Inc.,  OptiPlex 9020M\n{micro}","A14, dated 06/27/2017","Intel Corporation 8 Series/C220","SSD","Core(TM) i5-4590T |  4c",6144,"4096, 4096","Xeon E3-1200 v3/4th Gen","i915","Linux Mint 19.3","xfce4","Xfwm4","lightdm","4.19.106-rt46-lcnc","quiet splash","intel_idle","blacklisted","loaded","0 |  0","2.8.0",7197,64,-44.5,42,2,"no parport","no parport","no parport"]
[{"$nulls":3},68,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=250#211401",20200930,"2021-06-06","Yes |\nYes","Dell Inc.,  OptiPlex 980","A18, dated 02/27/2018","Intel Corporation 5 Series/3400 Series ","SSD","Core(TM) i5 CPU         650",4096,"4096, 4096","Core Processor Integrated Graphics Controller","i915","Debian GNU/Linux 10 (buster)","??? {SF?}","e16","lightdm","5.10.41-rt42-xanmod1","quiet isolcpus=1 mitigations=off intel_idle.max_cstate=0 pr\nocessor.max_cstate=0 idle=poll acpi_irq_nobalance noirqbalance","none","loaded","loaded","0 |  0","2.8.1",7202,42,-6.9,6.9,0.4,-9.4,9.3,0.3]
[{"$nulls":3},69,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=250#212460",20200930,"2021-06-20","Probably Yes |  No parport","Dell Inc.,  OptiPlex 790","A11, dated 12/30/2011","Intel Corporation 6 Series/C200","SSD","Core(TM) i5-2400",6144,"4096, 4096, 4096, 4096","2nd Generation Core Processor Family Integrated Graphics Controller","i915","Debian GNU/Linux 10 (buster)","xfce4","Xfwm4","lightdm","4.19.0-11-rt-amd64","??? {SF?}","intel_idle","loaded","loaded","0 |  0","2.8.1",7204,73,-71,83.6,3.4,"no parport","no parport","no parport"]
[{"$nulls":3},70,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=250#222359",20200930,"2021-10-06","No |  \nNo Parport","FUJITSU,  FUTRO S720","V4.6.5.4 R1.15.0 for D3313-B1x, dated 11/06/2014","?","SSD","AMD GX-217GA SOC with Radeon(tm) HD Graphics",1024,4096,"Kabini [Radeon HD 8280E]","radeon","Debian GNU/Linux 10 (buster)","gnome","Xfwm4","lightdm","4.19.0-17-rt-amd64","quiet","acpi_idle","blacklisted","blacklisted","0 |  0","2.8.2.11.g6a3d0a434","1204  | \n{Rt-error}",43.5,-178.4,214.4,13.7,"no parport","no parport","no parport"]
[{"$nulls":3},71,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=260#224630",20200930,"2021-10-14","Yes |\nYes","ITX-ASRock880GXH","P1.30, dated 05/04/2018","?","SSD","Celeron(R) J4005 | 2 c",4096,4096,"UHD Graphics 605","Post says nomodeset removes driver","Linux Mint 20.2","lightdm","Xfwm4","lightdm","5.10.0-0.bpo.8-rt-amd64","quiet splash nomodeset isolcpus=1","intel_idle","blacklisted","blacklisted","0 |  0","2.8.2.52.ga5f8e5cc0",7203,49,-15.6,16.2,0.6,-23.5,24.3,0.3]
[{"$nulls":3},72,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=260#233326",20200930,"2022-01-27","Yes w. Isolcpu=1 |\nNo parport","LENOVO,  10MR00xxxx\n{Thinkcentre M710q Tiny i3-7100T}","M1AKT28A, dated 09/13/2017","Intel Corporation 200 Series/Z370","SSD","Core(TM) i3-7100T |\n2c",3072,"single 8 GiB DDR4 SO-DIMM","HD Graphics 630","i915","Debian GNU/Linux 11 (bullseye)","lightdm","Xfwm4","lightdm","5.10.0-11-rt-amd64","quiet","intel_idle","blacklisted","blacklisted","0 |  0","2.9-pre (7b27504b…)"," 1238 |\nManual termination",58,"-117.3 |\n-80 w. isolcpu=1","116.9 |\n80 w. isolcpu=1",11.3,"no parport","no parport","no parport"]
[{"$nulls":3},73,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=260#233799",20200930,"2022-02-02","Yes |  \nNo parport","Intel Corporation,  NUC7i5BNH","BNKBL357.86A.0087.2021.1210.1903, dated 12/10/2021","?","SSD","Core(TM) i5-7260U |\n1 c",4096,"8192, 8192","Intel Corporation","i915","Debian GNU/Linux 10 (buster)","xfce4","Xfwm4","lightdm","4.19.0-18-rt-amd64","quiet transparent_hugepage=never splash mitigations=off isolcpus=1 acpi_irq_nobalance noirqbalance lapic nohlt idle=poll radeon.modeset=0 intel_idle.max_cstate=0 processor.max_cstate=0 ipv6.disable=1 pci=routeirq","none","blacklisted","blacklisted","0 |  0","2.8.2.11.g6a3d0a434",7204,55,-83.7,86.4,4.8,"no parport","no parport","no parport"]
[{"$nulls":3},74,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=280#236739",20200930,"2022-03-09","Probably Yes |  Probably Yes","Dell Inc.,  OptiPlex 980  ","A18, dated 02/27/2018","Intel Corporation 5 Series/3400","SSD","Core(TM) i5 CPU         650 | \n2 c",4096,"2048, 2048, 2048, 2048","Core Processor Integrated Graphics Controller","i915","Debian GNU/Linux 10 (buster)","gnome","Xfwm4","lightdm","5.10.0-0.bpo.9-rt-amd64","quiet isolcpus=1 ","intel_idle","loaded","blacklisted","0 |  0","2.8.2.11.g6a3d0a434","249  | \n{Rt-error}",61,-10.1,10.2,0.6,-14.6,21.8,0.2]
[{"$nulls":3},75,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=280#236754",20200624,"2022-03-08","Probably No {too short a test} |  Probably Yes","SAMSUNG ELECTRONICS CO., LTD., QX310/QX410/QX510/SF310/SF410/SF510","03MX.M005.20101011.SCY, dated 10/11/2010","Intel Corporation 5 Series/3400","SSD"," Core(TM) i5 CPU M 480 |\n2 c",3072,"4096, 4096","GT218M [GeForce 310M] |\nCore Processor Integrated Graphics Controller","Nouveau |\nI915","Linux Mint 18.1","??? {SF?}","??? {SF?}","??? {SF?}","4.8.11-rt7","quiet splash","intel_idle","blacklisted","loaded","0 |  0","2.8.0~pre1","9  | \n{Rt-error}","??? {SF?}",-23.2,24,1.3,-24.6,56,1.1]
[{"$nulls":3},76,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=280#236824",20200930,"2022-03-10","Yes |  \nNo parport","ASUSTeK COMPUTER INC.,  All Series","2601, dated 12/08/2014","Intel Corporation 9","SSD","Core(TM) i7-4790K CPU | \n4 c",8192,"8192, 8192","Xeon E3-1200 v3/4th Gen","i915","Debian GNU/Linux 10 (buster)","gnome","Xfwm4","lightdm","4.19.0-19-rt-amd64","quiet splash","intel_idle","blacklisted","loaded","0 |  0","2.9.0~pre0.5982.gcebd57f65",7202,60,-30.4,30.3,0.7,"no parport","no parport","no parport"]
[{"$nulls":3},77,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=280#236826",20200930,"2022-03-10"," Yes |  \n Yes","Dell Inc.,  OptiPlex 980  ","A18, dated 02/27/2018","Intel Corporation 5 Series/3400","SSD","Core(TM) i5 CPU         650 | \n2 c",4096,"2048, 2048, 2048, 2048","Core Processor Integrated Graphics Controller","i915","Debian GNU/Linux 10 (buster)","kdeconnectd","Kwin","lightdm","4.19.0-19-rt-amd64","quiet isolcpus=1 mitigations=off intel_idle.max_cstate=0 processor.max_cstate=0 idle=poll acpi_irq_nobalance noirqbalance","intel_idle","blacklisted","blacklisted","0 |  0","2.8.2.11.g6a3d0a434",7204,63,-12.3,12.3,0.5,-18.3,15.5,0.2]
[{"$nulls":3},78,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=300#238144",20200930,"2022-03-23","Yes |  \nNo parport","ASUSTeK Computer INC.,  Maximus Extreme","1302, dated 03/24/2009","?","rotational","Core(TM)2 Quad  CPU   Q9550 |\n4 c",6144,"2048, 2048, 2048, 2048","RV710 [Radeon HD 4350/4550]","radeon","Debian GNU/Linux 10 (buster)","xfce4","Xfwm4","lightdm","4.19.0-19-rt-amd64","quiet splash  isolcpus=3 idle=poll","none","loaded","blacklisted","0 |  0","2.8.2.11.g6a3d0a434",7202,51,-6.1,6.2,0.2,"no parport","no parport","no parport"]
[{"$nulls":3},79,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=300#240319","20200930 {mod}","2022-04-15"," Yes |  \n Yes","ASUSTeK Computer INC.,  System Product Name","2801, dated 08/23/2010","?","rotational","Quad-Core AMD Opteron(tm) Processor 1354",512,"2048, 2048","RS780C [Radeon 3100]","radeon","Debian GNU/Linux 10 (buster)","gnome","Metacity (Marco)","lightdm","4.19.195-rtai-amd64","Command line: BOOT_IMAGE=/boot/vmlinuz-4.19.195-rtai-amd64 root=UUID=4073631f-841a-4052-937d-db13e0ebdbd0 ro idle=poll isolcpus=3 irqaffinity=1,2\n{SF?}","{SF?}","loaded","loaded","0 |  0","2.8.2.",7205,64,-13.4,13.6,0.3,-18.1,18.7,0.3]
[{"$nulls":3},80,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=300#240334","20200930 {mod}","2022-04-15"," Yes |  \n Yes","BIOSTAR Group,  A870U3","080015, dated 03/23/2012","?","rotational","AMD Phenom(tm) II X6 1035T\n6c ",512,"4096, 4096, 4096, 8192","RV710 [Radeon HD 4350/4550]","radeon","Debian GNU/Linux 10 (buster)","gnome","Metacity (Marco)","lightdm","4.19.195-rtai-amd64","BOOT_IMAGE=/boot/vmlinuz-4.19.195-rtai-amd64 root=UUID=325c60e8-39a5-47e1-b946-95e90ca3be25 ro idle=poll isolcpus=5 irqaffinity=1,2,3,4","{SF?}","loaded","loaded","0 |  0","2.8.2.",7201,"??? {SF?}",-5,5,0.1,-5.4,5.9,0.2]
[{"$nulls":3},81,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=320#248143 ",20200930,"2022-07-23"," Yes |  \n Yes","ASRock,  To Be Filled By O.E.M.","P1.90, dated 05/21/2018","?","SSD","Intel(R) Celeron(R) CPU J3355 |\n2 c",1024,"8192, 8192","??\n{SF?}","radeon | \ni915","Debian GNU/Linux 10 (buster)","xfce4","Xfwm4","lightdm","4.19.0-16-rt-amd64","quiet isolcpus=1 nohalt irqaffinity=0","intel_idle","loaded","loaded","0 |  0","2.8.2.",1801,50,-5.4,5.4,0.2,-6,6.6,0.2]
[{"$nulls":3},82,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=320#248552",20200930,"2022-07-28","Probably Yes |  \nNo parport ","LENOVO,  10MQS36600 {M710q}","M1AKT52A, dated 12/24/2021","?","SSD","Core(TM) i5-6400T | \n4 c",6144,"4096, 4096","HD Graphics 530","i915","Debian GNU/Linux 11 (bullseye)","gnome","Mutter (Muffin)","lightdm","5.10.0-16-rt-amd64","quiet isolcpus=1 noirqbalance mitigations=off nohlt idle=pool splash resume=UUID=73f68a61-1146-4abd-a9f9-d0f93ea00eb9","intel_idle","blacklisted","blacklisted","0 |  0","2.9.0~pre0.",7194,60,-113.9,106,11.4,"no parport","no parport","no parport"]
[{"$nulls":3},83,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=320#252004",20200930,"2022-09-15","Yes |  \nNo parport","{ThinkCentre M910Q}","M1AKT56A, dated 07/27/2022","Intel Corporation 200 Series/Z370","SSD","Core(TM) i5-6500T | \n4 c",6144,"8192, 16384","HD Graphics 530","i915","Debian GNU/Linux bookworm/sid","lightdm","Xfwm4","lightdm","5.19.0-1-rt-amd64","quiet isolcpus=2,3","intel_idle","blacklisted","blacklisted","0 |  0","{2.}9.0~pre0+git20220906.02744cdef6-1",3599,57,-48.3,45,3.5,"no parport","no parport","no parport"]
[{"$nulls":3},84,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=340#272535",20200930,"2023-05-30","No |  \nNo Parport","AWOW,  PC BOX","1.05, dated 03/06/2020","?","SSD","Celeron(R) CPU J3455 | 4c",1024,"1536, 1536, 1536, 1536\n{true???}","HD Graphics 500","i915","Debian GNU/Linux 12 (bookworm)","lightdm","Xfwm4","lightdm","6.3.0-rt11-linuxcnc","quiet isolcpus=2,3","acpi_idle","loaded","loaded","0 |  0","2.9.0~pre1.868.g22bebc47d","3561 | \n{Rt-error}",68,-986.5,915.1,2.6,"no parport","no parport","no parport"]
[{"$nulls":3},85,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=360#274288",20200930,"2023-06-26","Yes |  \nNo parport","HARDKERNEL,  ODROID-H2","1.23, dated 04/08/2021","?","SSD","Celeron(R) CPU J3455 | 4c",4096,"4096, 4096","GeminiLake [UHD Graphics 600]","i915","Debian GNU/Linux 12 (bookworm)","lightdm","Xfwm4","lightdm","6.1.0-9-rt-amd64","quiet isolcpus=2,3,4","intel_idle","blacklisted","blacklisted","0 |  0","2.9.0~pre1.934.g17208cd63",7205,55,-89.5,89.9,3.3,"no parport","no parport","no parport"]
[{"$nulls":3},86,"https://forum.linuxcnc.org/18-computer/39371-results-of-latency-test-list-of-computers-tested-for-use-with-linuxcnc?start=370#287524",20200930,"2023-12-08","Yes |  \nNo parport","ASUSTeK COMPUTER INC.,  PRIME J4005I-C","1801, dated 06/13/2022","?","SSD","Celeron(R) J4005 |\n2 c",4096,4096,"GeminiLake [UHD Graphics 600]","i915","Debian GNU/Linux 12 (bookworm)","lightdm","Xfwm4","lightdm","6.5.0-0.deb12.1-rt-amd64","quiet","none","blacklisted","blacklisted","0 |  0","2.9.1",7203,70,-88.8,92,2.6,"no parport","no parport","no parport"]
[{"$nulls":3},87]
[{"$nulls":3},88]
[{"$nulls":3},89]
[{"$nulls":3},90]
[{"$nulls":3},91]
[{"$nulls":3},92]
[{"$nulls":3},93]
[{"$nulls":3},94]
[{"$nulls":3},95]
[{"$nulls":3},96]
[{"$nulls":3},97]
[{"$nulls":3},98]
[{"$nulls":3},99]
[{"$nulls":3},100]
[{"$nulls":3},101]
[{"$nulls":3},102]
[{"$nulls":3},103]
[{"$nulls":3},104]
[{"$nulls":3},105]
[{"$nulls":3},106]
[{"$nulls":3},107]
[{"$nulls":3},108]
[{"$nulls":3},109]
[{"$nulls":3},110]
[{"$nulls":3},111]
[{"$nulls":3},112]
[{"$nulls":3},113]
[{"$nulls":3},114]
[{"$nulls":3},115]
[{"$nulls":3},116]
[{"$nulls":3},117]
[{"$nulls":3},118]
[{"$nulls":3},119]
[{"$nulls":3},120]
[{"$nulls":3},121]
[{"$nulls":3},122]
[{"$nulls":3},123]
[{"$nulls":3},124]
[{"$nulls":3},125]
[{"$nulls":3},126]
[{"$nulls":3},127]
[{"$nulls":3},128]
[{"$nulls":3},129]
[{"$nulls":3},130]
[{"$nulls":3},131]
[{"$nulls":3},132]
[{"$nulls":3},133]
[{"$nulls":3},134]
[{"$nulls":3},135]
[{"$nulls":3},136]
[{"$nulls":3},137]
[{"$nulls":3},138]
[{"$nulls":3},139]
[{"$nulls":3},140]
[{"$nulls":3},141]
[{"$nulls":3},142]
[{"$nulls":3},143]
[{"$nulls":3},144]
[{"$nulls":3},145]
[{"$nulls":3},146]
[{"$nulls":3},147]
[{"$nulls":3},148]
[{"$nulls":3},149]
[{"$nulls":3},150]
[{"$nulls":3},151]
[{"$nulls":3},152]
[{"$nulls":3},153]
[{"$nulls":3},154]
[{"$nulls":3},155]
[{"$nulls":3},156]
[{"$nulls":3},157]
[{"$nulls":3},158]
[{"$nulls":3},159]
[{"$nulls":3},160]
[{"$nulls":3},161]
[{"$nulls":3},162]
[{"$nulls":3},163]
[{"$nulls":3},164]
[{"$nulls":3},165]
[{"$nulls":3},166]
[{"$nulls":3},167]
[{"$nulls":3},168]
[{"$nulls":3},169]
[{"$nulls":3},170]
[{"$nulls":3},171]
[{"$nulls":3},172]
[{"$nulls":3},173]
[{"$nulls":3},174]
[{"$nulls":3},175]
[{"$nulls":3},176]
[{"$nulls":3},177]
[{"$nulls":3},178]
[{"$nulls":3},179]
[{"$nulls":3},180]
[{"$nulls":3},181]
[{"$nulls":3},182]
[{"$nulls":3},183]
[{"$nulls":3},184]